here is a dll for Gnss solutions to improve the HRMS+ VRMS values (and solve the issue you have with the Italian cadastre).

Please :

* go to  C:\Program Files\GNSS Solutions\App\
* remove the GSLS.dll
* copy the attached file (new GSLS.dll file) in this directory